

**Saflok™ Carabiner**

**Model: 2000112**

11/16 in. (17.5mm) gate opening steel carabiner with self closing/locking gate.



### PRODUCT HIGHLIGHTS

* 11/16 in. (17.5mm) gate opening steel carabiner
* Self closing and locking gate for added safety
* Highly corrosion resistant plated hardware
* High strength steel construction
* User friendly compact and lightweight design

SPECIFICATIONS

|  |  |
| --- | --- |
| **Attachment Type Info** | Hook |
| **Install Type** | Reusable |
| **Capacity** | 310 lbs. (141 kg) ANSI / 420 lbs. (190 kg) OSHA |
| **Brand** | DBI-SALA® |
| **Sub Brand** | Saflok™ |
| **Velocity Ship** | Yes |
| **iSafe Equipped** | No |
| **Label** | Stamped |
| **Model** | 2000112 |
| **Other Standards** | OSHA 1910.66, OSHA 1926.502, ANSI Z359.1 |
| **Physical Dimensions** | 4.33x2.66x0.75 (in) |
| **Physical Weight** | 0.60 lbs (0.3kg) |
| **Product Styles** | Fixed |
| **Product Types** | Carabiner |
| **Standards** | CSA Z259.12, Capital Safety Gen. Mfg. Req. |